Inspection Checklist (based on Bronco6g OP repetitive feedback):
Mechanical
· [bookmark: _GoBack]Pulley rub/ proximity next to radiator hose
· Coolant hose clamp tight
· Battery terminals tight (negative loose)
· Turbo Charge Air Cooler Hose securely attached to the Charge Air Cooler Pipe (these are the big black tubes in the engine compartment)
· Roll all windows up at once
· Check window auto-drop for excessive snag/wobble.  Reset windows by holding switches down for 10 secs.
· Tailgate hinge area and fuel door has paint issues
· Fluids all full (oil, washer, brake)
· Confirm SEVEN Quarts of oil filled, not six. It's a 7 qt pan with a 6 qt dipstick. Ref: https:///forum/threads/bronco-team-engineering-confirms-7-0-quarts-for-2-7l-engine-oil-change-is-correct.29047/
· Strut on the back window unglued from the hardtop
· Check all three bolts in the fuse box for looseness
· Alternator belt installed backwards (smooth side against pulley)
· Transfer case wire harness rubbing against drive shaft (missing plastic clamp)
Paint/Exterior
· MIC Hardtop rough/sharp edges, gaps, leaks, roof rattles, popping from guide pins, latches...especially seal in middle
· MIC panels all match in color, not two-tone
· MIC Panels contacting, rubbing body panels, especially around rear corner panels/tailgate.  Source of squeaks.
· Paint bubbles/paint defects
· Paint overspray on windshield and body panels.  (Rough to touch vs. baby/glass smooth)
· Missing paint in door jambs/door brackets (may need to remove doors to see hinges in jambs), tailgate, fuel door
· Body panel alignment
· Hood dents on passenger side caused by excessive panel bond on cross bars
· No license plate mounting (if mounting alternate location)
· Check underneath for corrosion
· Check for discoloration of trim MIC top due to long stay in outdoor storage
· Check for transport damage

Interior
· Test all roof latches (some missing)
· Check seat stitching and ensure seats match
· Check seat belt webbing for defects
· Sound deadening installed (hardliner)
· Interior and trunk lights/bulbs work
· Owner’s Manual and Tool kit in glovebox
· Any TSBs/ Service Alerts? A-pillar leak TSB: 21-2403
· Whistling mirrors
· Ensure floor mats are as ordered (Raptor/Warthog/Ranger logo mats installed in Bronco)
Miscellaneous
· Door bags
· Mismatched roll bars...holes drilled on one, but not the other
· Ensure all cameras work
· Check windshield washer bottle neck for zip-tie support (should not be there)
· Test Windshield Wiper reservoir is full and sprays fluid on windshield




Dealer Signature:_________________________________________ Date: _______________



Owner Signature: ________________________________________ Date: _______________

